{T} 877.294.3580 • {F} 516.294.0444 • {E} info@WTShade.com • 77 Second Avenue • Garden City Park, New York 11040 • www.WTShade.com

**SHORT FORM SPECIFICATIONS**

**WT SHADE® HELIARISE® MANUAL SHADES WITH OPTIONAL FASCIA**

1. Basis of Design- WT Shade® HeliaRise® SoloMount® brackets with optional front and/or rear fascia (color choices are: White (-10), Ivory (-04), Silver (-20), Bronze (-50), or Black (-90)). Brackets and other components will be color matched in either White (-10) or Black (-90) based on the fabric color. *See Color Coordination Guide at* [www.wtshade.com](http://www.wtshade.com) . Contact WT Shade at (877) 294- 3580.
2. All clutches and idle ends to have metal attachment points for security and clutch will be physically attached to the mounting bracket with an integrated safety hold-down screw.
3. Brackets will have mounting flange configured to wall, ceiling, or jamb mount applications with in-field reconfiguration possible. *See drawings for details.*
4. Chains to be #10 Stainless Steel with 100 lb. tensile strength.
5. Fabric to be specifier’s choice of EcoFabrix® [www.ecofabrix.com/products](http://www.ecofabrix.com/products) , Mermet [www.mermetusa.com](http://www.mermetusa.com) , or Phifer [www.phifer.com/sun-control/interior](http://www.phifer.com/sun-control/interior).

