{T} 877.294.3580 • {F} 516.294.0444 • {E} info@WTShade.com • 77 Second Avenue • Garden City Park, New York 11040 • www.WTShade.com

**SHORT FORM SPECIFICATIONS**

**WT SHADE® MOTORISE® MOTORIZED PIGGYBACK SHADES FOR LINE VOLTAGE**

**WITH OPTIONAL FASCIA**

1. Basis of Design- WT Shade® MotoRise® Piggyback SoloMount® brackets with optional front and/or rear fascia (color choices for fascia are: White (-10), Ivory (-04), Silver (-20), Bronze (-50), or Black (-90)). Brackets and other components will be color coordinated in either White (-10) or Black (-90) based on the fabric color. *See Color Coordination Guide at* [www.wtshade.com](http://www.wtshade.com) *.* Shading system will have 2 shades mounted in a staggered position. Contact WT Shade at (877) 294- 3580.
2. Brackets to have integrated retainer ring to securely attach motor and brackets. Spring-loaded idle end.
3. Brackets will have mounting flange configured to wall, ceiling, or jamb mount applications with in-field reconfiguration possible. *See drawings for details.*
4. Motors to be line voltage and controlled via Specifiers choice of controls including hand held remote control, wall switch or by integration into 3rd party control systems.
5. Fabric to be specifier’s choice of EcoFabrix® [www.ecofabrix.com/products](http://www.ecofabrix.com/products) , Mermet [www.mermetusa.com](http://www.mermetusa.com) , or Phifer [www.phifer.com/sun-control/interior](http://www.phifer.com/sun-control/interior). 