{T} 877.294.3580 • {F} 516.294.0444 • {E} info@WTShade.com • 77 Second Avenue • Garden City Park, New York 11040 • www.WTShade.com

**SHORT FORM SPECIFICATIONS**

**WT SHADE® MOTORISE® MOTORIZED SHADES FOR LINE VOLTAGE**

**WITH SLIM BRACKETS**

1. Basis of Design- WT Shade® MotoRise® Slim Brackets- Brackets will be Zinc Plated (-49).[www.wtshade.com/product-category/shading-systems/motorise/](http://www.wtshade.com/product-category/shading-systems/motorise/) .Contact WT Shade at (877) 294- 3580.
2. Brackets to have integrated retainer ring to securely attach motor and brackets. Spring-loaded idle end.
3. Brackets will have mounting flange configured to wall, ceiling, or jamb mount applications with in-field reconfiguration possible. *See drawings for details.*
4. Motors to be line voltage and controlled via specifier’s choice of controls including hand held remote control, wall switch or by integration into 3rd party control systems.
5. Fabric to be specifier’s choice of EcoFabrix® [www.ecofabrix.com/products](http://www.ecofabrix.com/products) , Mermet [www.mermetusa.com](http://www.mermetusa.com) , or Phifer [www.phifer.com/sun-control/interior](http://www.phifer.com/sun-control/interior). 